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Multiple Choice
Choose the answer that best answers each statement or question.
_______ 1. Which type of welding is also known as stick welding and has the welder use an electrode?

A. metal inert gas welding


B. stringer metal arc welding

C. tungsten inert gas welding


D. shielded metal arc welding

_______ 2. Which type of shielded metal arc welding machine is a simple transformer that plugs into normal 220V wiring?

A. DC (direct current) machine


B. simple electrode welding machine

C. AC (alternating current) machine


D. simple household welding machine

_______ 3. Which type of shielded metal arc welding machine acts as an electrical generator?

A. DC (direct current) machine


B. stringer metal arc welding machine

C. AC (alternating current) machine


D. metal inert gas welding machine

_______ 4. Which type of welding uses a combination of electricity and an inert shielding gas?

A. metal inert gas welding


B. AC shielded metal arc gas welding

C. DC shielded metal arc gas welding


D. AC/DC shielded metal arc gas welding

_______ 5. Which type of welding is used in situations where high quality results are essential?

A. metal inert gas welding


B. stringer metal arc welding

C. tungsten inert gas welding


D. shielded metal arc welding

_______ 6. What code means that the electrode is usable in any welding position?

A. “1”


B. “3”

C. “2”


D. “4”

_______ 7. The electrode should be kept at about a _____.

A. 5- to 20-degree angle from perpendicular in the direction of travel

B. 15- to 30-degree angle from perpendicular in the direction of travel

C. 20- to 45-degree angle from perpendicular in the direction of travel

D. 45- to 60-degree angle from perpendicular in the direction of travel

_______ 8. Oxygen cylinders are usually _____.

A. red


B. black

C. blue


D. green

_______ 9. Acetylene cylinders are usually _____.

A. red


B. black

C. blue


D. green

_______ 10. What part of cutting equipment is color coded red or black and supplies gas from the cylinder to the torch?

A. oxygen hose


B. acetylene hose

C. torch head


D. oxygen tube

_______ 11. What part of cutting equipment is attached to the cylinder outlet to control gas pressure to the torch?

A. torch head


B. oxygen check valve

C. oxygen regulator


D. oxygen cylinder valve

_______ 12. The oxygen hose is color coded _____.

A. red


B. black

C. blue


D. green

_______ 13. Goggles used for oxyfuel cutting must have a _____.

A. No. 1 or darker-shaded lens


B. No. 3 or darker-shaded lens

C. No. 2 or darker-shaded lens


D. No. 4 or darker-shaded lens

_______ 14. What type of fuel gas is often used on farms and in rural areas since it is easily accessible and less expensive than other fuels?

A. propane


B. natural gas

C. MAPP® gas


D. acetylene

_______ 15. What type of fuel gas is the most versatile for gas welding operations?

A. propane


B. natural gas

C. MAPP® gas


D. acetylene

_______ 16. What type of fuel gas is used mostly in industry?

A. propane


B. natural gas

C. MAPP® gas


D. acetylene

_______ 17. In the oxyfuel cutting process, the temperature of the metal must be between _____.

A. 800° F and 1000° F to burn


B. 1200° F and 1600° F to burn

C. 1000° F and 1200° F to burn


D. 1600° F and 1800° F to burn

_______ 18. The correct type of flame for heating, cutting, and welding with oxyfuel equipment is called a(n) _____.

A. neutral flame


B. carburizing flame

C. oxidizing flame


D. median flame

_______ 19. What type of flame for heating, cutting, and welding with oxyfuel equipment has excess oxygen in the mixture and is hotter than other flames?

A. neutral flame


B. carburizing flame

C. oxidizing flame


D. median flame

_______ 20. What type of flame for heating, cutting, and welding with oxyfuel equipment has excess gas in the mixture and is cooler than other flames?

A. neutral flame


B. carburizing flame

C. oxidizing flame


D. median flame

True or False
Indicate if each statement is true or false.
_______ 21. AC (alternating current) shielded metal arc welding machines are relatively expensive and suited for special purposes.

_______ 22. Shielded metal arc welding machines do not allow the user to set the amperage level.

_______ 23. The amount of time that a welder can be used before it must be allowed to cool down is called the duty cycle.

_______ 24. The simplest type of bead is called a stringer bead.

_______ 25. The acetylene cylinder valve can be opened fully at all times.

_______ 26. Oxygen is a colorless, odorless, tasteless gas.

_______ 27. Oxygen is an extremely flammable gas.

_______ 28. When using oxyfuel equipment, backfire is a condition in which the torch flame momentarily burns back into the tip.

_______ 29. When using oxyfuel equipment, flashback occurs when the flame burns back into the torch body.

_______ 30. When using oxyfuel equipment, flashback is characterized by a loud snap or pop.

_______ 31. When cutting steel, a cut made with too much cutting oxygen pressure will leave a top edge uneven or dished.

_______ 32. When cutting steel, a cut made with too much preheat will result in the top edge of the cut being flared.

_______ 33. When cutting steel, a quality cut has clean and square edges on the top and bottom and the surface of the cut is smooth with uniform vertical drag lines that bend back slightly at the bottom.

_______ 34. If flashback occurs when using oxyfuel equipment, it will generally correct without any action from the operator.

Matching
Identify electrode code markings by matching it with its number.
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_______ 35. welding position

_______ 36. indication it is for electric arc welding

_______ 37. special characteristics

_______ 38. tensile strength
Matching

Match each term with its definition.

A.
flux


B.
slag


C.
electrode

D.
electrode holder

E.
ground clamp

_______ 39. metal welding rod

_______ 40. a device that grips the electrode

_______ 41. provides a gas shield for the molten pool during the welding process

_______ 42. a device attached by a cable to the arc welder

_______ 43. layer created by impurities that float to the top of the weld

Matching

Match each piece of oxyfuel cutting equipment with its definition.

A.
coupling nut


B.
cutting head


C.
mixing chamber

D.
oxygen cutting lever

E.
oxygen preheat valve

_______ 44. depressing this allows oxygen to travel through the oxygen tube

_______ 45. controls the supply of oxygen from the supply hose

_______ 46. designed to accept different types of cutting tips

_______ 47. oxygen and fuel gas are mixed within this tube

_______ 48. used to connect the cutting attachment securely to the torch handle

Short Answer
49. What are the two methods of establishing an arc?

_____________________________________________________________________________________

_____________________________________________________________________________________

_____________________________________________________________________________________

50. What is oxidation?
_____________________________________________________________________________________

_____________________________________________________________________________________

_____________________________________________________________________________________

51. What are the two basic steps in the oxyfuel cutting process?

_____________________________________________________________________________________

_____________________________________________________________________________________

_____________________________________________________________________________________
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