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Multiple Choice
Choose the answer that best completes each statement or question.
_______ 1. Which governmental agency regulates safe practices to prevent work-related injuries, illnesses, and deaths?

A.
USDA


B.
FDA


C.
OSHA

D.
OSSA

_______ 2. What can ensure safety in the shop?

A.
common sense


B.
good judgment


C.
behaving responsibly

D.
all of the above

_______ 3. Most injuries that occur in the shop or elsewhere are the result of _____.

A.
machinery


B.
electricity


C.
human error

D.
unknown causes

_______ 4. Machinery is a source of hazard when it is _____.

A.
running


B.
operated improperly
C.
foreign made

D.
old

_______ 5. Machinery should only be used with proper _____.

A.
skill


B.
knowledge


C.
ability

D.
all of the above

_______ 6. Keeping the shop clean and organized can prevent injury from _____.

A.
falling objects


B.
tripping


C.
spills

D.
all of the above

_______ 7. You should never look at the welding arc without proper eye protection, which is a shaded lens ranging in number from _____.

A.
No. 1 to No. 3


B.
No. 3 to No. 6


C.
No. 6 to No. 9

D.
No. 9 to No. 12

_______ 8. A material is considered flammable if it has a flash point of less than _____.

A.
100° F


B.
130° F


C.
175° F

D.
212° F

_______ 9. Which class of fire occurs in ordinary combustible materials such as wood, rags, and rubbish?

A.
Class A


B.
Class B


C.
Class C

D.
Class D

_______ 10. Which class of fire is fueled by flammable metals, such as magnesium?

A.
Class A


B.
Class B


C.
Class C

D.
Class D

_______ 11. Which class of fire is fueled by flammable liquids such as gasoline, oil, grease, paints, and thinners?

A.
Class A


B.
Class B


C.
Class C

D.
Class D

_______ 12. Which class of fire consists of electrical fires that occur in or near electrical equipment?

A.
Class A


B.
Class B


C.
Class C

D.
Class D

_______ 13. Which class of fire may be extinguished with water?

A.
Class A


B.
Class B


C.
Class C

D.
Class D

_______ 14. Water can help to spread rather than stop fires that are _____.

A.
Class A


B.
Class B


C.
Class C

D.
Class D

_______ 15. The use of water can result in electric shock or electrocution in fires that are _____.

A.
Class A


B.
Class B


C.
Class C

D.
Class D

True or False
Indicate if each statement is true or false.
_______ 16. Behaving responsibly is the best way to keep from causing an accident that could injure yourself or an innocent bystander.

_______ 17. Even a small electric shock is painful, while standard household current can kill.

_______ 18. The type of PPE is the same for all types of agricultural work.

_______ 19. Synthetic material should be worn when welding.

_______ 20. Many fire extinguishers are designed to fight multiple classes of fire.

_______ 21. Use fire extinguishers occasionally to make sure they work.

Matching
Match each PPE with its purpose.

A.
safety glasses


B.
coveralls


C.
rubber boots

D.
steel-toed boots

E.
clear face shields

_______ 22. protects the entire face from flying particles or liquid splashes

_______ 23. protects the feet from water and mild chemicals

_______ 24. protects the feet from falling objects

_______ 25. protects the eyes

_______ 26. protects the body, arms, and legs from dust and flying debris

Matching

Match each PPE with its purpose.

A.
gloves


B.
respirators


C.
dust masks

D.
ear plugs or ear muffs

E.
helmets and shaded face shields

_______ 27. protects the hearing from loud or continuous noise

_______ 28. protects you from breathing dirt particles
_______ 29. protects the face and eyes from heat, harmful rays, and hot metal when working

_______ 30. protects the hands from splinters, hot or sharp metal, and chemicals

_______ 31. protects you from breathing toxic gases, fumes, and harmful fibers

Matching

Match each safety color code with its description.

A.
red


B.
blue


C.
green

D.
yellow

E.
orange

F.
black and white

G.
purple or black and yellow

_______ 32. designates radiation hazards

_______ 33. used to designate safety and first-aid equipment

_______ 34. used to designate traffic movement and housekeeping areas

_______ 35. used to identify fire protection equipment and apparatus, and to designate “danger” or “stop”

_______ 36. used to warn against starting equipment, moving equipment, or using equipment under repair or being worked on

_______ 37. used to designate dangerous parts of machinery and parts of equipment that can cause electric shock

_______ 38. used to designate caution and mark physical hazards such as stumbling, falling, tripping, striking against, and caught-between

Completion
Write a word in each blank that best completes each sentence.
39. Wear appropriate _____________________ that fits properly.

40. Remove _______________ and dangling _______________ , and tie back long _______________.

41. Keep the shop and work area ___________________ and well ___________________.
42. Only use tools for their specific ___________________.
43. Know the location and proper use of ___________________ ___________________.
44. Repair or replace all worn or frayed ___________________ cords.

45. Never touch metal that could be ___________________.
Short Answer
46. What should you do before beginning a weld?

_____________________________________________________________________________________

_____________________________________________________________________________________

_____________________________________________________________________________________

_____________________________________________________________________________________

47. What should you do to avoid electrical shock when welding?

_____________________________________________________________________________________

_____________________________________________________________________________________

_____________________________________________________________________________________

_____________________________________________________________________________________
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