|  |
| --- |
| OKLAHOMA CORPORATION COMMISSION – PETROLEUM STORAGE TANK DIVISION **P. O. Box 52000, Oklahoma City, OK 73152-2000**  **(405) 521-4683** |

# GROUNDWATER MONITORING WELL RELEASE DETECTION

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## FOR CALENDAR YEAR FACILITY NAME FACILITY I. D. NUMBER

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **\_\_\_\_\_\_\_\_\_\_**

**FACILITY ADDRESS CITY (MONITORING DEVICE)**

MONITORING PERFORMED BY: OPERATOR □ CONTRACTOR □ NAME AND LICENSE NO: \_\_\_\_\_\_\_\_\_\_

CONTRACTOR ADDRESS\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ CITY\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ZIP\_\_\_\_\_\_\_\_\_\_\_\_\_ PHONE\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |
| --- |
| SITE MAP (Indicate **North** on map; include building, tank pit area and pump islands; identify each Monitor Well by a distinct number)  **OAC 165:25-3-6.24 Requires that a site-specific site assessment must be conducted and approved by the OCC prior to using this method of release detection. The monitoring device must be able to detect at least 1/8 inch of free product.** |

**REPORT 1/8 INCH FREE PRODUCT WITHIN 24 HOURS TO 405-521-4683**

**MONITORING WELL DATA: Use Additional Pages for Additional Wells**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date Inspected** | **MW #\_\_\_\_\_\_** | | **MW #\_\_\_\_\_\_** | | **MW #\_\_\_\_\_\_** | | **MW #\_\_\_\_\_\_\_** | |  | |  |
| **Free Product**  **(In inches)** | **Depth to**  **Groundwater** | **Free Product**  **(In inches)** | **Depth to Groundwater** | **Free Product**  **(In inches)** | **Depth to Groundwater** | **Free Product (in inches)** | **Depth to**  **Groundwater** | **Legible Signature** |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |

##### TOTAL NUMBER OF WELLS BEING MONITORED: \_\_\_\_\_\_\_\_\_\_\_\_ PAGE \_\_\_\_ OF \_\_\_\_ PAGES