|  |
| --- |
| OKLAHOMA CORPORATION COMMISSION – PETROLEUM STORAGE TANK DIVISION**P. O. Box 52000, Oklahoma City, OK 73152-2000****(405) 521-4683** |

# Year\_\_\_\_\_\_\_\_\_\_ INVENTORY RECONCILIATION RELEASE DETECTION

# Cycle Start Date\_\_\_\_\_\_\_\_\_\_\_ Cycle End Date\_\_\_\_\_\_\_\_\_

## FACILITY I. D. NUMBER FACILITY NAME TANK # FUEL TYPE

**\_\_\_\_0.2 Gal Per Hour Tank Test, CSLD, SCALD, via ATG every 30 days WATER CHECK DATE\_\_\_\_\_\_\_INCHES\_\_\_\_\_\_\_**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Date | **(1)****Start Stick Inventory (Gallons)** | **(2)****Gallons Delivered** | **(3)****Gallons Pumped****(Add percent sold through blend pump if applicable.)** | **(4)****Book Inventory (Gallons)** | Ending Stick Inventory**(5) | (6)****(Inches) | (Gallons)** | **(7)****Daily Over (+)****Or Short ( - )****(End – Book)** | **Initials** |
| **NOTE: Column numbers (1) + (2) -- (3) = (4) Column numbers (6) -- (4) = (7)** |
| **1** |  |  |  |  |  |  |  |  |
| **2** |  |  |  |  |  |  |  |  |
| **3** |  |  |  |  |  |  |  |  |
| **4** |  |  |  |  |  |  |  |  |
| **5** |  |  |  |  |  |  |  |  |
| **6** |  |  |  |  |  |  |  |  |
| **7** |  |  |  |  |  |  |  |  |
| **8** |  |  |  |  |  |  |  |  |
| **9** |  |  |  |  |  |  |  |  |
| **10** |  |  |  |  |  |  |  |  |
| **11** |  |  |  |  |  |  |  |  |
| **12** |  |  |  |  |  |  |  |  |
| **13** |  |  |  |  |  |  |  |  |
| **14** |  |  |  |  |  |  |  |  |
| **15** |  |  |  |  |  |  |  |  |
| **16** |  |  |  |  |  |  |  |  |
| **17** |  |  |  |  |  |  |  |  |
| **18** |  |  |  |  |  |  |  |  |
| **19** |  |  |  |  |  |  |  |  |
| **20** |  |  |  |  |  |  |  |  |
| **21** |  |  |  |  |  |  |  |  |
| **22** |  |  |  |  |  |  |  |  |
| **23** |  |  |  |  |  |  |  |  |
| **24** |  |  |  |  |  |  |  |  |
| **25** |  |  |  |  |  |  |  |  |
| **26** |  |  |  |  |  |  |  |  |
| **27** |  |  |  |  |  |  |  |  |
| **28** |  |  |  |  |  |  |  |  |
| **29** |  |  |  |  |  |  |  |  |
| **30** |  |  |  |  |  |  |  |  |
|  | (8) TOTAL GALLONS PUMPED- |  | **(9) TOTAL GALLONS OVER OR SHORT** |  |  |

Drop last 2 whole numbers from TOTAL GALLONS PUMPED Compare these numbers (9 &10)

and enter number on the line below

**LEAK CHECK: +130 gallons = \_\_\_\_\_\_\_\_ gallons (10)**

IF TOTAL GALLONS OVER/SHORT (#9) IS LARGER THAN LEAK CHECK + 130 (#10) FOR 2 CONSECUTIVE

30-DAY PERIODS REPORT TO OKLAHOMA CORPORATION COMMISSION WITHIN 24 HOURS

 (405) 521-4683

Revised February 2017